1. Configure IP addresses to router in Packet Tracer, explore the following messages

* Ping response
* Destination Unreachable
* Request Timeout
* Reply

2)







